H1 H2

L1 L2

*Feed dumped LF Feed dumped SF*

3 000\*

2 500

330

*Side view*

*\* Track widening kit*

***HEIGHT AND LENGTH***

|  |  |  |
| --- | --- | --- |
| Standard unit excluding all options and drill steel | Metric | Imperial |
| FlexiROC D60 andFlexiROC D65 LF | 23 700 kg (T3) | 52 250 lb |
| 24 100 kg (T4) | 53 130 lb |
|  | 22 600 kg (T3) | 49 820 lb |
| 23 000 kg (T4) | 50 700 lb |

***WEIGHT***

FlexiROC D60 and

|  |  |  |
| --- | --- | --- |
| Long Feed (LF) dumped | Metric | Imperial |
| Height (H1) | 3 500 mm | 11’ 6’’ |
| Length (L1) | 11 600 mm | 38’ |
| Short Feed (SF) dumped | Metric | Imperial |
| Height (H2) | 3 500 mm | 11’ 6’’ |
| Length (L2) | 11 350 mm | 37’ 2’’ |
| Feed height | Metric | Imperial |
| Long feed (LF) | 11 600 mm | 38’ |
| Short Feed (SF) | 9 400 mm | 31’ |

FlexiROC D65 SF